# Assembly notes Analog Control Board Rev. 1.0

All directions are relative to the PCI slot at the bottom.

-MMCX connectors: The connector slot is slightly too small, use a file to make it big enough.

-C17: Polarity marking is missing, right side is positive

-C18: Polarity marking is missing, top side is positive

-D1: Polarity marking is missing, right side is positive

-D2: Polarity marking is missing, right side is positive

-D3: Polarity marking is missing, right side is positive

-U5: Pin 1 marking is missing, pin 1 is top left

-U9: Pin1 marking is missing, pin 1 is top left. Footprint too big for SOIC8, but it will fit

-Y1: Pin 1 marking is missing, pin 1 is top right